#[
#       Name:           wm_DiffEngine_Patchprops.txt
#
#       Project:        Wavecom Machine Network Project: Insignia Patch Generation Tool Configuration File
#
#       Created On: January 2006
#
#       Version:        $Id:  $
#
#       Purpose:
#           Provide a template for the description of the metadata
#           properties to be used as required by the Insignia GenFOTO
#           FOTO library utility. Note that the name of this file itself is
#           not significant.
#
#           The exact usage/meaning of the properties that are specified
#           is defined in the "Standalone Difference Engine - User Guide"
#           document.
#
#       (c) Copyright Insignia Solutions plc, 2004
#       (c) Copyright Wavecom SA, 2006
#]


# Patch is Generated with GenFOTO tool from 2 images
# Images are generated from binary files with GenDevImg tool
#
# -- Properties file definition assumed by GenFOTO utilities --

# MANDATORY flash-geometry
# Flash geometry where the package will be downloaded
# Liste of region definitions {N blocks, Block size in bytes}, {N, Size}, etc.
# Wavecom comments: Depends on module Flash architecture. Mutch match the actual module flash size,
# else will be rejected by UA
# Typical block size used: 0x2000 (8 kB), 0x10000 (64 kB)
flash-geometry:{512,0x20000}

# OPTIONAL  compression-type:   zlib | paq
# Must match the agent. Zlib is more efficient
# Wavecom comments: Zlib is used
compression-type: zlib

# OPTIONAL  foto-digest-type    Adler32 | md5
# Digest checksum algorithm to verify the integrity of the Update Package by the Update Agent
# Must fit the UA implementation
# Md5 more efficient, Adler32 lighter for small embedded devices
# Wavecom comments: Md5 is already used by OMA client
foto-digest-type: md5

# OPTIONAL  image-digest-type   Adler32 | md5
# Digest checksum algorithm to verify that both images before and after patch install are correct
# Must fit the UA implementation
# Md5 more efficient, Adler32 lighter for small embedded devices
# Wavecom comments: Md5 is already used by OMA client
image-digest-type: md5

# OPTIONAL  restartmap-type     4bpb | 2bpb | none
# Defines the data format within the Update agent used for the agent to ensure restartability
# in case of power loss during patch install
#   4bpb: default, ok for any NOR flash including multi bit cell NOR (Intel's StrataFlash)
#   2bpb: (smaller) for single bit cell NOR
#   none: NAND
# Wavecom comments: 4bpb is the only one supported by the UA. DO NOT USE OTHER
restartmap-type: none

# OPTIONAL  generator-type      Generic | Data16 | THUMBv1_BE | THUMBv1_LE | THUMBv2_BE | THUMBv2_LE | MCORE_BE
# Defines the Generator type to be used by the update package generator process
# Should not be used.
# Wavecom comments: General purpose, let the Generator select the low-level generator from the Image metadata information
# The one that should be used is THUMBv1_LE
# test 26/02/2006 with Generic: on X51 & X55 versions = no change, THUMBv1_LE automatically selected
#generator-type: THUMBv1_LE






